--- a/doc/mpdconf.example
+++ b/doc/mpdconf.example
@@ -10,14 +10,14 @@
 # be disabled and audio files will only be accepted over ipc socket (using
 # file:// protocol) or streaming files over an accepted protocol.
 #
-#music_directory		"~/music"
+music_directory		"/sdcard/Music"
 #
 # This setting sets the MPD internal playlist directory. The purpose of this
 # directory is storage for playlists created by MPD. The server will use
 # playlist files not created by the server but only if they are in the MPD
 # format. This setting defaults to playlist saving being disabled.
 #
-#playlist_directory		"~/.mpd/playlists"
+playlist_directory		"~/.mpd/playlists"
 #
 # This setting sets the location of the MPD database. This file is used to
 # load the database at server start up and store the database while the
@@ -25,7 +25,7 @@
 # MPD to accept files over ipc socket (using file:// protocol) or streaming
 # files over an accepted protocol.
 #
-#db_file			"~/.mpd/database"
+db_file			"~/.mpd/database"
 
 # These settings are the locations for the daemon log files for the daemon.
 #
@@ -35,7 +35,7 @@
 # If you use systemd, do not configure a log_file.  With systemd, MPD
 # defaults to the systemd journal, which is fine.
 #
-#log_file			"~/.mpd/log"
+log_file			"~/.mpd/log"
 
 # This setting sets the location of the file which stores the process ID
 # for use of mpd --kill and some init scripts. This setting is disabled by
@@ -43,19 +43,19 @@
 #
 # If you use systemd, do not configure a pid_file.
 #
-#pid_file			"~/.mpd/pid"
+pid_file			"~/.mpd/pid"
 
 # This setting sets the location of the file which contains information about
 # most variables to get MPD back into the same general shape it was in before
 # it was brought down. This setting is disabled by default and the server
 # state will be reset on server start up.
 #
-#state_file			"~/.mpd/state"
+state_file			"~/.mpd/state"
 #
 # The location of the sticker database.  This is a database which
 # manages dynamic information attached to songs.
 #
-#sticker_file			"~/.mpd/sticker.sql"
+sticker_file			"~/.mpd/sticker.sql"
 #
 ###############################################################################
 
@@ -85,12 +85,12 @@
 #bind_to_address		"any"
 #
 # And for Unix Socket
-#bind_to_address		"~/.mpd/socket"
+bind_to_address		"@TERMUX_PREFIX@/var/run/mpd.socket"
 #
 # This setting is the TCP port that is desired for the daemon to get assigned
-# to.
+# to. Normally this is 6600 but for termux this port needs to be above 8000.
 #
-#port				"6600"
+#port				"8600"
 #
 # Suppress all messages below the given threshold.  Use "verbose" for
 # troubleshooting. Available setting arguments are "notice", "info", "verbose",
@@ -135,12 +135,12 @@
 # If this setting is set to "yes", MPD will discover audio files by following
 # symbolic links outside of the configured music_directory.
 #
-#follow_outside_symlinks	"yes"
+follow_outside_symlinks	"yes"
 #
 # If this setting is set to "yes", MPD will discover audio files by following
 # symbolic links inside of the configured music_directory.
 #
-#follow_inside_symlinks		"yes"
+follow_inside_symlinks		"yes"
 #
 ###############################################################################
 
@@ -213,28 +213,6 @@
 # blocks. Setting this block is optional, though the server will only attempt
 # autodetection for one sound card.
 #
-# An example of an ALSA output:
-#
-#audio_output {
-#	type		"alsa"
-#	name		"My ALSA Device"
-##	device		"hw:0,0"	# optional
-##	mixer_type      "hardware"	# optional
-##	mixer_device	"default"	# optional
-##	mixer_control	"PCM"		# optional
-##	mixer_index	"0"		# optional
-#}
-#
-# An example of an OSS output:
-#
-#audio_output {
-#	type		"oss"
-#	name		"My OSS Device"
-##	device		"/dev/dsp"	# optional
-##	mixer_type      "hardware"	# optional
-##	mixer_device	"/dev/mixer"	# optional
-##	mixer_control	"PCM"		# optional
-#}
 #
 # An example of a shout output (for streaming to Icecast):
 #
@@ -265,7 +243,8 @@
 #	type		"recorder"
 #	name		"My recorder"
 #	encoder		"vorbis"		# optional, vorbis or lame
-#	path		"/var/lib/mpd/recorder/mpd.ogg"
+##  for termux changed "path" to somewhere on android that works
+#	path		"~/mpd.ogg" 
 ##	quality		"5.0"			# do not define if bitrate is defined
 #	bitrate		"128"			# do not define if quality is defined
 #	format		"44100:16:1"
@@ -285,6 +264,14 @@
 #	max_clients	"0"			# optional 0=no limit
 #}
 #
+# An example of a pulseaudio output
+#
+audio_output {
+	type		"pulse"
+	name		"PulseAudio Output"
+	enabled		"no"
+}
+#
 # An example of a pulseaudio output (streaming to a remote pulseaudio server)
 #
 #audio_output {
@@ -295,56 +282,31 @@
 ##	media_role	"media_role"		#optional
 #}
 #
-# An example of a winmm output (Windows multimedia API).
-#
-#audio_output {
-#	type		"winmm"
-#	name		"My WinMM output"
-##	device		"Digital Audio (S/PDIF) (High Definition Audio Device)" # optional
-#		or
-##	device		"0"		# optional
-##	mixer_type	"hardware"	# optional
-#}
-#
-# An example of a wasapi output (Windows multimedia API).
-#
-#audio_output {
-#	type		"wasapi"
-#	name		"My WASAPI output"
-##	device		"Digital Audio (S/PDIF) (High Definition Audio Device)" # optional
-#		or
-##	device		"0"		# optional
-##	mixer_type	"hardware"	# optional
-## Exclusive mode blocks all other audio source, and get best audio quality without resampling.
-##	exclusive	"no"		# optional
-## Enumerate all devices in log.
-##	enumerate	"no"		# optional
-#}
+# An example of an opensl android output.
+audio_output {
+        type            "sles"
+        name            "OpenSLES output"
+        mixer_type      "software"
+}
 #
 # An example of an openal output.
 #
-#audio_output {
-#	type		"openal"
-#	name		"My OpenAL output"
-##	device		"Digital Audio (S/PDIF) (High Definition Audio Device)" # optional
-#}
-#
-# An example of an sndio output.
-#
-#audio_output {
-#	type		"sndio"
-#	name		"sndio output"
-#	mixer_type	"hardware"
-#}
-#
-# An example of an OS X output:
-#
-#audio_output {
-#	type		"osx"
-#	name		"My OS X Device"
-##	device		"Built-in Output"	# optional
-##	channel_map      "-1,-1,0,1"	# optional
-#}
+audio_output {
+	type		"openal"
+	name		"OpenAL output"
+	mixer_type	"software"
+	device		"OpenSL"
+	enabled		"no"
+}
+#Fifo output for visualizations in ncmpcpp
+audio_output {
+        type            "fifo"
+        name            "ncmpcpp visualizer"
+        path            "@TERMUX_PREFIX@/var/run/mpd.fifo"
+        format          "44100:16:2"
+	enabled		"no"
+}
+
 #
 ## Example "pipe" output:
 #
