Created by, or sourced from, K11MCH1
https://github.com/K11MCH1/freedreno_turnip-CI/commit/db9f6d0b31bbabe3fef22e3682015764cd73eb5e
Adreno 710-only variant also discovered in KreitinnSoftware's repo here:
https://github.com/KreitinnSoftware/MiceWine-RootFS-Generator/commit/6e9d54ab5d280821922c1e8a7a02d84ba1621cbc
Upstream issue:
https://gitlab.freedesktop.org/mesa/mesa/-/issues/13036

--- a/src/freedreno/common/freedreno_devices.py
+++ b/src/freedreno/common/freedreno_devices.py
@@ -1065,6 +1065,42 @@ add_gpus([
         raw_magic_regs = a730_raw_magic_regs,
     ))
 
+add_gpus([
+        GPUId(chip_id=0x07010000, name="FD710"), # KGSL, no speedbin data
+        GPUId(chip_id=0xffff07010000, name="FD710"), # Default no-speedbin fallback
+    ], A6xxGPUInfo(
+        CHIP.A7XX,
+        [a7xx_base, a7xx_gen1],
+        num_ccu = 4,
+        tile_align_w = 64,
+        tile_align_h = 32,
+        num_vsc_pipes = 32,
+        cs_shared_mem_size = 32 * 1024,
+        wave_granularity = 2,
+        fibers_per_sp = 128 * 2 * 16,
+        highest_bank_bit = 16,
+        magic_regs = a730_magic_regs,
+        raw_magic_regs = a730_raw_magic_regs,
+    ))
+
+add_gpus([
+        GPUId(chip_id=0x43020000, name="FD720"), # KGSL, no speedbin data
+        GPUId(chip_id=0xffff043020000, name="FD720"), # Default no-speedbin fallback
+    ], A6xxGPUInfo(
+        CHIP.A7XX,
+        [a7xx_base, a7xx_gen1],
+        num_ccu = 4,
+        tile_align_w = 64,
+        tile_align_h = 32,
+        num_vsc_pipes = 32,
+        cs_shared_mem_size = 32 * 1024,
+        wave_granularity = 2,
+        fibers_per_sp = 128 * 2 * 16,
+        highest_bank_bit = 16,
+        magic_regs = a730_magic_regs,
+        raw_magic_regs = a730_raw_magic_regs,
+    ))
+
 add_gpus([
         GPUId(chip_id=0x07030001, name="FD730"), # KGSL, no speedbin data
         GPUId(chip_id=0xffff07030001, name="FD730"), # Default no-speedbin fallback
--- a/src/freedreno/drm-shim/freedreno_noop.c
+++ b/src/freedreno/drm-shim/freedreno_noop.c
@@ -237,6 +237,16 @@ static const struct msm_device_info device_infos[] = {
       .chip_id = CHIPID(6, 6, 0, 0xff),
       .gmem_size = 1024 * 1024 + 512 * 1024,
    },
+   {
+      .gpu_id = 710
+      .chip_id = 0x07010000,
+      .gmem_size = 2 * 1024 * 1024,
+   },
+   {
+      .gpu_id = 720
+      .chip_id = 0x43020000,
+      .gmem_size = 2 * 1024 * 1024,
+   },
    {
       .gpu_id = 730,
       .chip_id = 0x07030001,
